Camera update manual V1.1.5
1.Input the Camera IP or IP range if need to update more cameras at the same time,and then click Add .
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2.Select the Firmware that need to update and click Update
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3.Wait for the update process finish.
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